EnergyPLAN version
16.0
EnergyUnit=
TWh/year
CapacityUnit=
MW
MonetaryUnit=
EUR
Input_el_demand_Twh=
30.77
Input_El_demand_elec_heating_share=
0
Input_El_demand_cooling_share=
0
input_dh_demand_TWh=
0
input_RES1_capacity=
25000
input_RES2_capacity=
0
input_RES1_factor=
0
input_RES2_factor=
0.7
input_RES3_capacity=
19500
input_RES3_factor=
0
input_RES4_capacity=
0
input_RES4_factor=
0
NameRES1=
Wind
NameRES2=
Offshore Wind
NameRES3=
Photo Voltaic
NameRES4=
River Hydro
input_dh_ann_gr1=
0
input_dh_ann_gr2=
0
input_dh_ann_gr3=
10.21
input_solar_ann_gr1=
0
input_solar_ann_gr2=
0
input_solar_ann_gr3=
0.33
input_cshp_th_gr1=
0
input_cshp_th_gr2=
0
input_cshp_th_gr3=
0
input_AddExport_TWh=
0
input_flexible_day_TWh=
3.42
input_flexible_week_TWh=
0
input_flexible_4weeks_TWh=
0
input_flexible_day_max=
532.81
input_flexible_week_max=
1
input_flexible_4weeks_max=
1
input_cshp_el_gr1=
0
input_cshp_el_gr2=
0
input_cshp_el_gr3=
0
input_cshp_el_gr3=
0
Filnavn_elbehov=
GRC Electricity demand.txt
Filnavn_individual_heatdemand=
IT Individual heating demand 2050 0.85.txt
Filnavn_cooling_demand=
GRC Cooling demand.txt
Filnavn_individual_solar=
GRC Solar thermal.txt
Filnavn_dh=
IT District heating demand 2050 0.85.txt
input_button_add_subtract=
No
input_button_add2=
No
Filnavn_AddExport=
EL Fixed import-export.txt
Filnavn_wind=
GRC Offshore wind.txt
Filnavn_wave=
GR Onshore wind.txt
Filnavn_solar=
GRC Solar thermal.txt
Filnavn_cshp=
const.txt
Filnavn_pv=
GR Solar PV.txt
Filnavn_RES4=
GRC Solar PV.txt
filnavn_hydro_water=
EL Hydro water.txt
filnavn_nuclear=
const.txt
input_transport_TWh=
16
input_transport_TWh_V2G=
6.22
Filnavn_transport=
EL Transport demand.txt
Filnavn_transport_V2G=
EL Transport demand.txt
Filnavn_transport_H2=
EL Transport demand.txt
input_km_diesel=
1.5
input_km_ngas=
1.5
input_km_biomass=
1.5
input_km_h2=
3
input_km_ev=
5
input_km_v2g=
5
input_V2G_MaxShare=
0.2
input_V2G_Cap_Charge=
38423.75
input_V2G_ConnectionShare=
0.7
input_V2G_Eff_Charge=
0.9
input_V2G_Eff_Inv=
0.9
input_V2G_Battery=
64.04
input_V2G_Cap_Inv=
1921.19
input_cap_chp2_el=
0
input_eff_chp2_el=
0.4
input_eff_chp2_th=
0.5
input_cap_hp2_el=
0
input_eff_hp2_cop=
3
input_cap_boiler2_th=
0
input_eff_boiler2_th=
0.9
input_cap_chp3_el=
1377
input_eff_chp3_el=
0.45
input_eff_chp3_th=
0.45
input_cap_hp3_el=
275.4
input_eff_hp3_cop=
4
input_cap_boiler3_th=
4300.8
input_eff_boiler3_th=
0.95
input_cap_pp_el=
5000
input_hydro_cap=
3392
input_hydro_eff=
0.95
input_hydro_watersupply=
6.15
input_hydro_storage=
2456
input_hydro_pump_cap=
0
input_hydro_pump_eff=
0.9
input_nuclear_cap=
0
input_nuclear_eff=
0.39
input_eff_pp_el=
0.55
input_eff_dhp_th=
0.9
input_storage_gr2_cap=
0
input_storage_gr3_cap=
1800
input_FixedBoiler2=
0
input_FixedBoiler3=
0
input_regulation=
2
input_marketmodel=
1
input_chpgr3_cap_minimum=
0
input_hp_maxload=
0.5
input_imp_reg_fac=
0
input_exp_pp_reg_fac=
9999
input_exp_chp_reg_fac=
9999
Filnavn_prices=
const.txt
input_exp_hp_reg_fac=
9999
input_max_imp_exp=
0
input_lost_value=
0
input_nordpool_add_fac=
0
input_nordpool_mult_fac=
2
input_keol_reg=
234500000
input_depend_fac=
0
input_import_bottleneck_addprice_factor=
150
input_stabilisation_share_min=
0
input_stabilisation_share_chp2=
0
input_RES1_stab_share=
0
input_RES2_stab_share=
0
input_RES3_stab_share=
0
input_RES4_stab_share=
0
input_fuel_dhp[1]=
0
input_fuel_dhp[2]=
0
input_fuel_dhp[3]=
0
input_fuel_dhp[4]=
0
input_fuel_chp2[1]=
0
input_fuel_chp2[2]=
0
input_fuel_chp2[3]=
0
input_fuel_chp2[4]=
0
input_fuel_chp3[1]=
0
input_fuel_chp3[2]=
0
input_fuel_chp3[3]=
0.75
input_fuel_chp3[4]=
0.25
input_fuel_Boiler2[1]=
0
input_fuel_Boiler2[2]=
0
input_fuel_Boiler2[3]=
0
input_fuel_Boiler2[4]=
0
input_fuel_Boiler3[1]=
0
input_fuel_Boiler3[2]=
0
input_fuel_Boiler3[3]=
0.75
input_fuel_Boiler3[4]=
0.25
input_fuel_PP[1]=
0
input_fuel_PP[2]=
0
input_fuel_PP[3]=
0.75
input_fuel_PP[4]=
0.25
input_fuel_Transport[1]=
0
input_fuel_Transport[2]=
0
input_fuel_Transport[3]=
0
input_fuel_Transport[4]=
0
input_fuel_Transport[6]=
0
input_VC_boiler_dh=
3.4
input_VC_chp_dh=
3.05
input_VC_hp_dh=
3.9
input_VC_pp=
2.74
input_VC_hydro=
4
Input_VC_eh_dh=
1
input_VC_geothermal=
0
input_VC_electrolyser=
0
input_VC_pump=
0
input_VC_turbine=
0
input_VC_boiler_indv=
0
input_VC_chp_indv=
0
input_VC_hp_indv=
0
input_VC_eh_indv=
0
input_fuel_Households[1]=
0
input_fuel_Households[2]=
0
input_fuel_Households[3]=
0
input_fuel_Households[4]=
1.1998838039081
input_HH_coalboiler_eff=
0.97
input_HH_oilboiler_eff=
0.97
input_HH_ngasboiler_eff=
0.98
input_HH_bioboiler_eff=
0.79
input_HH_H2CHP_eff_th=
0.98
input_HH_NgasCHP_eff_th=
0.5
input_HH_BioCHP_eff_th=
0.5
input_HH_H2CHP_heat=
0
input_HH_NgasCHP_heat=
0
input_HH_H2CHP_solar=
0
input_HH_NgasCHP_solar=
0
input_HH_BioCHP_solar=
0
input_HH_HP_solar=
1.70623476915732
input_HH_EB_solar=
0
input_HH_BioCHP_heat=
0
input_HH_HP_heat=
8.53117384578662
input_HH_EB_heat=
0.947908205087402
input_HH_H2CHP_eff_el=
0
input_HH_NgasCHP_eff_el=
0
input_HH_BioCHP_eff_el=
0
input_HH_HP_COP=
3
input_HH_H2CHP_storage=
0
input_HH_NgasCHP_storage=
0
input_HH_BioCHP_storage=
0
input_HH_HP_storage=
0
input_HH_EB_storage=
0
input_HH_H2CHP_CapLimit=
1
input_HH_NgasCHP_CapLimit=
1
input_HH_BioCHP_CapLimit=
1
input_HH_HP_CapLimit=
1
input_fuel_CSHP[1]=
0
input_fuel_CSHP[2]=
0
input_fuel_CSHP[3]=
0
input_fuel_CSHP[4]=
5.1
input_fuel_Various[1]=
0
input_fuel_Various[2]=
0
input_fuel_Various[3]=
0
input_fuel_Various[4]=
0
input_fuel_CO2[1]=
95
input_fuel_CO2[2]=
74
input_fuel_CO2[3]=
56.7
input_fuel_price[1]=
2.9
input_fuel_price[2]=
10.4
input_fuel_price[3]=
6.6
input_fuel_price[4]=
6.6
input_Handling_Cen[1]=
0.18
input_Handling_Cen[2]=
0.3
input_Handling_Cen[3]=
0.27
input_Handling_Cen[4]=
3.66
input_Handling_Dec[1]=
0
input_Handling_Dec[2]=
1.18
input_Handling_Dec[3]=
0.86
input_Handling_Dec[4]=
3.95
input_Handling_Indv[1]=
0
input_Handling_Indv[2]=
3.3
input_Handling_Indv[3]=
2.19
input_Handling_Indv[4]=
6.45
input_fuel_price[6]=
14.9
input_Handling_Transp[2]=
3.3
input_Handling_Transp[3]=
1.59
input_Handling_Transp[4]=
0
input_Tax_Indv[1]=
0
input_Tax_Indv[2]=
0
input_Tax_Indv[3]=
0
input_Tax_Indv[4]=
0
input_Tax_Indu[1]=
0
input_Tax_Indu[2]=
0
input_Tax_Indu[3]=
0
input_Tax_Indu[4]=
0
input_Tax_Boiler[1]=
0
input_Tax_Boiler[2]=
0
input_Tax_Boiler[3]=
0
input_Tax_Boiler[4]=
0
input_Tax_CHP[1]=
0
input_Tax_CHP[2]=
0
input_Tax_CHP[3]=
0
input_Tax_CHP[4]=
0
input_CO2_price=
42
input_Maintain_price=
0
Input_Button_Price=
No
Input_Button_Coal=
Variable
Input_Button_oil=
Variable
Input_Button_Ngas=
Variable
Input_Button_Biomass=
Variable
input_fuel_pp[6]=
0
input_fuel_chp2[6]=
0
input_fuel_Boiler2[6]=
0
input_fuel_pp2[6]=
0
input_fuel_chp3[6]=
0
input_fuel_Boiler3[6]=
0
input_cap_ELTtrans_el=
6000
input_eff_ELTtrans_fuel=
0.7
input_cap_eltCHPindv_el=
0
input_eff_eltCHPindv_fuel=
0.64
input_cap_pump_el=
1010.91
input_eff_pump_el=
0.8
input_cap_turbine_el=
1010.91
input_eff_turbine_el=
0.8
input_fuel_dhp[6]=
0
input_H2storage_gr3_cap=
0
input_H2storage_trans_cap=
106
input_H2storage_CHPindv_cap=
0
input_storage_pump_cap=
10.11
input_CAES_fuel_ratio=
0
TS_input[1]=
0
TS_input[2]=
0
TS_input[3]=
0
TS_input[4]=
0
TS_input[5]=
0
TS_input[6]=
0
TS_input[7]=
0
TS_input[8]=
0
TS_input[9]=
0
Input_Cooling_el_demand=
4.8301
Input_Cooling_DHgr1_Heatdemand=
0
Input_Cooling_DHgr2_Heatdemand=
0
Input_Cooling_DHgr3_Heatdemand=
1.2545
Input_Cooling_el_eff=
6.9784
Input_Cooling_DHgr1_eff=
2
Input_Cooling_DHgr2_eff=
2
Input_Cooling_DHgr3_eff=
0.7
Input_Tax_eh_dh=
0
Input_Tax_hp_dh=
0
Input_Tax_elt_dh=
0
Input_Tax_eh_indv=
0
Input_Tax_hp_indv=
0
Input_Tax_elt_indv=
0
Input_Tax_cars_indv=
0
input_Interest=
3
input_Inv_solar_dh=
325
input_Period_solar_dh=
30
input_FOM_solar_dh=
0
input_Inv_CHP2=
0
input_Period_CHP2=
0
 input_FOM_CHP2=
0
input_Inv_HP2=
0
input_Period_HP2=
0
 input_FOM_HP2=
0
input_Inv_Heatstorage2=
3
input_Period_Heatstorage2=
20
 input_FOM_Heatstorage2=
0.5
input_Inv_CHP3=
1.35
input_Period_CHP3=
25
 input_FOM_CHP3=
3.3
input_Inv_HP3=
2.13
input_Period_HP3=
25
 input_FOM_HP3=
0.3
input_Inv_Heatstorage3=
52
input_Period_Heatstorage3=
30
 input_FOM_Heatstorage3=
0
input_Inv_Boilers_dh=
0.23
input_Period_Boilers_dh=
25
input_FOM_Boilers_dh=
3.55
input_Inv_PP=
1.35
input_Period_PP=
25
input_FOM_PP=
3.3
input_Inv_Wind=
0.96
input_Period_Wind=
27
input_FOM_Wind=
1.3
input_Inv_WindOffshore=
1.78
input_Period_WindOffshore=
27
input_FOM_WindOffshore=
1.9
input_Inv_PV=
0.35
input_Period_PV=
30
input_FOM_PV=
2.5
input_Inv_Wave=
0
input_Period_Wave=
0
input_FOM_Wave=
0
input_Inv_RiverOffHydro=
0
input_Period_RiverOffHydro=
0
input_FOM_RiverOffHydro=
0
input_Inv_HydroPower=
2.76
input_Period_HydroPower=
80
input_FOM_HydroPower=
1.15
input_Inv_HydroStorage=
7.5
input_Period_HydroStorage=
50
input_FOM_HydroStorage=
1.5
input_Inv_HydroPump=
0.6
input_Period_HydroPump=
50
input_FOM_HydroPump=
1.5
input_Inv_Nuclear=
7.94
input_Period_Nuclear=
40
input_FOM_Nuclear=
1.4
input_Inv_Geothermal=
5.53
input_Period_Geothermal=
30
input_FOM_Geothermal=
1.4
input_Inv_Electrolyser=
0.5
input_Period_Electrolyser=
25
input_FOM_Electrolyser=
5
input_Inv_HydrogenStorage=
15.06
input_Period_HydrogenStorage=
48
input_FOM_HydrogenStorage=
1.37
input_Inv_Pump=
0
input_Period_Pump=
0
input_FOM_Pump=
0
input_Inv_Turbine=
0
input_Period_Turbine=
0
input_FOM_Turbine=
0
input_Inv_PumpStorage=
175
input_Period_PumpStorage=
80
input_FOM_PumpStorage=
1
input_Inv_Boilers_indv=
5.9
input_Period_Boilers_indv=
20
input_FOM_Boilers_indv=
7.42
input_Inv_CHP_indv=
4
input_Period_CHP_indv=
20
input_FOM_CHP_indv=
5.45
input_Inv_HP_indv=
5
input_Period_HP_indv=
18
input_FOM_HP_indv=
4.72
input_Inv_EB_indv=
2.5
input_Period_EB_indv=
30
input_FOM_EB_indv=
0.84
input_Inv_Various1=
192784
input_Period_Various1=
15
input_FOM_Various1=
1.16
input_Inv_Various2=
751
input_Period_Various2=
10
input_FOM_Various2=
0
input_Inv_Various3=
28922
input_Period_Various3=
30
input_FOM_Various3=
0
input_HH_coalboiler_SolarShare=
1
input_HH_oilboiler_SolarShare=
1
input_HH_ngasboiler_SolarShare=
1
input_HH_bioboiler_SolarShare=
1
input_HH_H2CHP_SolarShare=
1
input_HH_NgasCHP_SolarShare=
1
 input_HH_BioCHP_SolarShare=
1
 input_HH_HP_SolarShare=
1
 input_HH_EB_SolarShare=
1
 input_HH_coalboiler_Solar=
0
 input_HH_oilboiler_Solar=
0
 input_HH_ngasboiler_Solar=
0
 input_HH_bioboiler_Solar=
0
 Input_HH_coalboiler_Storage=
0
 Input_HH_oilboiler_Storage=
0
 Input_HH_Ngasboiler_Storage=
0
 Input_HH_Bioboiler_Storage=
0
input_solar_storage_gr1=
0
input_solar_storage_gr2=
0
input_solar_storage_gr3=
23.2
input_solar_share_gr1=
1
input_solar_share_gr2=
1
input_solar_share_gr3=
1
input_solar_loss_gr1=
0
input_solar_loss_gr2=
0
input_solar_loss_gr3=
0
input_VC_V2G=
0
input_Tax_CAES=
0
input_VC_HydroPump=
0
input_Tax_PumpCAES=
0
input_Inv_solar_indv=
0
input_Period_solar_indv=
0
input_FOM_solar_indv=
0
input_Period_Various4=
20
input_FOM_Various4=
0.6
input_Inv_Various4=
1749.64
input_Period_Various5=
0
input_FOM_Various5=
0
input_Inv_Various5=
0
input_Period_Various6=
0
input_FOM_Various6=
0
input_Inv_Various6=
0
input_fuel_price_alt1[1]=
0
input_fuel_price_alt1[2]=
0
input_fuel_price_alt1[3]=
0
input_fuel_price_alt1[4]=
0
input_fuel_price_alt2[1]=
0
input_fuel_price_alt2[2]=
0
input_fuel_price_alt2[3]=
0
input_fuel_price_alt2[4]=
0
input_km_petrol=
1.5
input_fuel_price[5]=
15
input_fuel_price_alt1[5]=
0
input_fuel_price_alt2[5]=
0
input_fuel_price_alt1[6]=
0
input_fuel_price_alt2[6]=
0
input_Handling_Transp[5]=
3.76
input_Handling_Transp[1]=
0.3
input_fuel_Transport[5]=
0
input_Period_Various7=
0
input_FOM_Various7=
0
input_Inv_Various7=
0
input_Period_Various8=
0
input_FOM_Various8=
0
input_Inv_Various8=
0
input_Period_Various9=
0
input_FOM_Various9=
0
input_Inv_Various9=
0
input_Period_Various10=
0
input_FOM_Various10=
0
input_Inv_Various10=
0
input_fuel_CO2[9]=
32.5
input_fuel_price[9]=
0
input_Handling_Cen[9]=
0
input_Handling_Dec[9]=
0
input_Tax_Indu[9]=
0
input_Tax_Boiler[9]=
0
input_Tax_CHP[9]=
0
input_fuel_price_alt1[9]=
0
input_fuel_price_alt2[9]=
0
input_Waste1_Waste=
0
input_Waste2_Waste=
0
input_Waste3_Waste=
7.6
input_Waste1_Eff_th=
0.8
input_Waste2_Eff_th=
0.8
input_Waste3_Eff_th=
0.5
input_Waste1_Eff_el=
0
input_Waste2_Eff_el=
0
input_Waste3_Eff_el=
0.3
input_Waste1_Eff_biofueltrans=
0
input_Waste2_Eff_biofueltrans=
0
input_Waste3_Eff_biofueltrans=
0
input_Waste1_Eff_biofuelCHP=
0
input_Waste2_Eff_biofuelCHP=
0
input_Waste3_Eff_biofuelCHP=
0
input_Waste1_Eff_various=
0
input_Waste2_Eff_various=
0
input_Waste3_Eff_various=
0
input_Waste1_price_various=
0
input_Waste2_price_various=
0
input_Waste3_price_various=
0
input_km_waste=
1.5
input_eh2=
0
input_eh3=
358.4
input_cap_pp2_el=
0
input_eff_pp2_el=
0.45
input_fuel_PP2[1]=
0
input_fuel_PP2[2]=
0
input_fuel_PP2[3]=
0
input_fuel_PP2[4]=
0
input_RSC_Waste=
0
input_RSC_Coal=
0
input_RSC_Biomass=
0
input_RSC_eff_fuel_M1=
0.6
input_RSC_eff_elec_M1=
0.1
input_RSC_eff_th_M1=
0.2
input_RSC_eff_fuel_M2=
0.2
input_RSC_eff_elec_M2=
0.2
input_RSC_eff_th_M2=
0.5
input_VC_RSC_M1=
0
input_VC_RSC_M2=
0
Button_WasteVar=
1.Coal/2.Biomass
input_Waste2_eff_th_geo=
0
input_Waste3_eff_th_geo=
0
input_Waste2_eff_el_geo=
0
input_Waste3_eff_el_geo=
0
input_Waste2_eff_steam=
0
input_Waste3_eff_steam=
0
input_Waste2_cop_GeoHP_steam=
0
input_Waste3_cop_GeoHP_steam=
0
input_Waste2_cap_steamstorage=
0
input_Waste3_cap_steamstorage=
0
input_Waste2_loss_steamstorage=
0
input_Waste3_loss_steamstorage=
0
input_Waste2_cop_GeoHP_steamstorage=
0
input_Waste3_cop_GeoHP_steamstorage=
0
Input_Button_PumpHydro=
No
Filnavn_waste=
const.txt
TS_input[10]=
0
TS_input[11]=
0
input_stabilisation_share_waste=
0
Various1Text=
Vehicles
Various2Text=
EV Charging stations
Various3Text=
Transport Infrastrucutre
Various4Text=
Industry - Efficiency Measure Costs
Various5Text=

Various6Text=

Various7Text=

Various8Text=
0.00
Various9Text=
0.00
Various10Text=
0.00
input_Inv_Waste_CHP=
201.25
input_Period_Waste_CHP=
25
input_FOM_Waste_CHP=
2.3
input_Inv_absorp_HP=
0
input_Period_absorp_HP=
0
input_FOM_absorp_HP=
0
input_Biogas_elec=
0.02
input_Biogas_dh1=
0
input_Biogas_dh2=
0
input_Biogas_dh3=
0
input_Biogas_prod=
3.59
Filnavn_Biogas_elec=
const.txt
Filnavn_Biogas_dh=
const.txt
Filnavn_Biogas_prod=
const.txt
Input_V2GRegulation=
1
input_km_LPG=
1.5
input_fuel_Transport[9]=
0
input_pp_cap_minimum=
0
Input_Button_IndvHPStorage=
Not active
input_GeoPower_cap=
0
input_GeoPower_eff=
0.1
filnavn_GeoPower=
const.txt
Filnavn_Gasi_dh=
const.txt
Input_GasiElecShare=
0.01
Input_GasiDH3Share=
0.05
Input_GasiBiomassInput=
24.5
Input_GasiSteamShare=
0.13
Input_GasiSteamEff=
1.25
Input_GasiColdgasEff=
0.9
Input_GasiCapInput=
0
Input_GasiUpgradeEff=
1
Input_BiogasUpgradeEff=
1
Input_BiogasWetBiomassInput=
3.59
Input_BiogasSolidBiomassInput=
0
Input_GasNetStorage=
0
Filnavn_Industry_Ngas=
const.txt
Filnavn_Transport_Ngas=
const.txt
input_button_BiogasBiomassOutput=
Biomass
input_Inv_Biogas=
196
input_Period_Biogas=
20
input_FOM_Biogas=
15
input_Inv_Gasi=
1.1
input_Period_Gasi=
20
input_FOM_Gasi=
2.5
input_fuel_price_alt1[10]=
0
input_fuel_price_alt2[10]=
0
input_fuel_price_alt1[11]=
0
input_fuel_price_alt2[11]=
0
input_fuel_price[10]=
8.8
input_fuel_price[11]=
0
input_Handling_BioCon[4]=
1.19
input_Handling_BioCon[10]=
0.91
input_Handling_BioCon[11]=
1.49
Filnavn_BioDiesel_Elec=
const.txt
Input_BioDieselInput=
0
Input_BioDieselElecShare=
0
Input_BioDieselShare=
0.4
Input_BioDieselBiomassShare=
0
input_HH_HP_StorageMaxCapLimit=
1
input_HH_HP_StorageMinCapLimit=
0.33
Filnavn_BioPetrol_dh=
const.txt
Input_BioPetrolElecShare=
0.01
Input_BioPetrolSteamShare=
0.12
Input_BioPetrolSteamEff=
1.25
Input_BioPetrolEff=
0.4
Input_BioPetrolFoodShare=
0.5
Input_BioPetrolFoodValue=
0
Input_BioPetrolDH3Share=
0.1
Input_BioPetrolInput=
0
input_stabilisation_share_V2G=
0
input_stabilisation_share_TransmissionLine=
0
Input_inv_BioDiesel=
1.45
Input_FOM_BioDiesel=
6.2
Input_Period_BioDiesel=
25
Input_Period_BioPetrol=
25
Input_FOM_BioPetrol=
6.2
Input_inv_BioPetrol=
1.45
Input_HeatPumpRegulation=
1
Filnavn_BioJP_dh=
const.txt
Input_BioJPElecShare=
0.01
Input_BioJPSteamShare=
0.12
Input_BioJPSteamEff=
1.25
Input_BioJPEff=
0.4
Input_BioJPFoodShare=
0
Input_BioJPFoodValue=
0
Input_BioJPDH3Share=
0
Input_BioJPInput=
0
Input_SynHydroSynGridGas=
0
Input_SynHydro_HydrogenShare=
0.36
Input_SynHydro_eff=
0.82
Input_SynHydro_MaxCapacity=
0
Input_CO2HydroMaxCapacity=
678
Input_CO2HydroSequestrationElecEff=
0.09
Input_CO2HydroSequestrationCO2Eff=
0.19
Input_CO2HydroSynGridGas=
0
Input_CO2HydroElectrolyserEff=
178.34
Input_SynDiesel=
3.87
Input_SynDiesel_eff=
1
Input_SynJP=
9.83
Input_SynJP_eff=
0.74
Input_SynPetrol=
0
Input_SynPetrol_eff=
1
input_GeoPower_factor=
1
input_Nuclear_factor=
1
input_fuel_price[12]=
1.75
input_fuel_price_alt1[12]=
0
input_fuel_price_alt2[12]=
0
input_fuel_CO2[8]=
59.64
input_fuel_price[8]=
0
input_fuel_price_alt1[8]=
0
input_fuel_price_alt2[8]=
0
Input_inv_BioJP=
1.78
Input_FOM_BioJP=
5.1
Input_Period_BioJP=
25
Input_inv_Tidal=
0
Input_FOM_Tidal=
0
Input_Period_Tidal=
0
Input_inv_CSP=
0
Input_FOM_CSP=
0
Input_Period_CSP=
0
Input_inv_CO2Hydro=
200
Input_FOM_CO2Hydro=
4.3
Input_Period_CO2Hydro=
20
Input_inv_SynHydro=
0.2
Input_FOM_SynHydro=
4
Input_Period_SynHydro=
25
Input_inv_SynFuel=
0.5
Input_FOM_SynFuel=
4
Input_Period_SynFuel=
25
Input_inv_BiogasUpgrade=
0.25
Input_FOM_BiogasUpgrade=
2.5
Input_Period_BiogasUpgrade=
15
Input_inv_GasificationUpgrade=
0
Input_FOM_GasificationUpgrade=
0
Input_Period_GasificationUpgrade=
0
Input_SynMethanSynGridGas=
0
Input_SynMethan_HydrogenShare=
0.37
Input_SynMethan_eff=
0.82
Input_SynMethan_MaxCapacity=
0
Input_NaturalCooling_DHgr1=
0
Input_NaturalCooling_DHgr2=
0
Input_NaturalCooling_DHgr3=
0.1631
Filnavn_naturalcooling_demand=
GRC Cooling demand.txt
Input_CO2Hydro_DHgr2_Share=
0
Input_CO2Hydro_DHgr3_Share=
0
Input_TransElt_DHgr2_Share=
0
Input_TransElt_DHgr3_Share=
0.05
Input_CO2HydroHydrogenRatio=
1.21
Filnavn_Freshwater=
const.txt
FreshWaterDemand=
0
input_FreshWaterStorageCapacity=
0
input_FreshWaterPumpEfficiency=
0.85
input_FreshWaterPumpCapacity=
0
input_DesalinationPlantCapacity=
0
input_DesalinationPlantEfficiency=
7
input_FreshWaterShare=
0.7
input_BrineShare=
0.3
input_DesalinationTurbineEfficiency=
0.9
input_DesalinationPumpEfficiency=
0.85
input_DesalinationTurbineCapacity=
0
input_DesalinationPumpCapacity=
0
input_BrineStorageCapacity=
0
input_BrineEnergyEquivalent=
2
Input_inv_Desalination=
0
Input_FOM_Desalination=
0
Input_Period_Desalination=
0
Input_inv_WaterStorage=
0
Input_FOM_WaterStorage=
0
Input_Period_WaterStorage=
0
input_CO2_CCS=
0
input_Inv_Boilers_dh_gr1=
0
input_Period_Boilers_dh_gr1=
0
input_FOM_Boilers_dh_gr1=
0
ThermalStorageDays=
14
input_HH_EB_CapLimit=
1
input_CCS_El_PerUnit=
0.37
input_CCS_Regulation_number=
1
Input_CCS_Capacity=
0
input_Heatdemand_PerHouse=
3470
input_Inv_EHgr2gr3=
0
input_Period_EHgr2gr3=
0
input_FOM_EHgr2gr3=
0
input_dh_ann_loss_gr1=
0.2
input_dh_ann_loss_gr2=
0.15
input_dh_ann_loss_gr3=
0.15
input_coal_ann_losses=
0
input_oil_ann_losses=
0
input_gas_ann_losses=
0
input_bio_ann_losses=
0
Various11Text=
0.00
Various12Text=
0.00
Various13Text=
0.00
Various14Text=
0.00
Various15Text=
EE improv
Various16Text=
Additional grid costs
Various17Text=
DH costs
Various18Text=
0.00
Various19Text=
0.00
Various20Text=
0.00
input_Period_Various11=
0
input_FOM_Various11=
0
input_Inv_Various11=
0
input_Period_Various12=
0
input_FOM_Various12=
0
input_Inv_Various12=
0
input_Period_Various13=
0
input_FOM_Various13=
0
input_Inv_Various13=
0
input_Period_Various14=
0
input_FOM_Various14=
0
input_Inv_Various14=
0
input_Period_Various15=
40
input_FOM_Various15=
0.5
input_Inv_Various15=
17993.3828336856
input_Period_Various16=
50
input_FOM_Various16=
0.1
input_Inv_Various16=
434.651001477777
input_Period_Various17=
40
input_FOM_Various17=
0.1
input_Inv_Various17=
6494.93553778162
input_Period_Various18=
0
input_FOM_Various18=
0
input_Inv_Various18=
0
input_Period_Various19=
0
input_FOM_Various19=
0
input_Inv_Various19=
0
input_Period_Various20=
0
input_FOM_Various20=
0
input_Inv_Various20=
0
Input_OilNetStorage=
0
Input_MethanolNetStorage=
0
Input_inv_GasNetStorage=
0
Input_FOM_GasNetStorage=
0
Input_Period_GasNetStorage=
0
Input_inv_OilNetStorage=
0
Input_FOM_OilNetStorage=
0
Input_Period_OilNetStorage=
0
Input_inv_MethanolNetStorage=
0
Input_FOM_MethanolNetStorage=
0
Input_Period_MethanolNetStorage=
0
Input_inv_Interconnection=
0
Input_FOM_Interconnection=
0
Input_Period_Interconnection=
0
input_cap_chp2_thermal=
1500
input_cap_chp3_thermal=
1500
input_geo_th_gr1=
0
input_geo_th_gr2=
0
input_geo_th_gr3=
0.421292535594401
Input_chp_thermal_cap_button=
Auto
input_ind_surplus_heat1=
0
input_ind_surplus_heat2=
0
input_ind_surplus_heat3=
2.08539303044092
Input_Inv_geo_th=
396.67
Input_FOM_geo_th=
0.83
Input_Period_geo_th=
30
Input_Inv_ind_surplus_heat=
30
Input_FOM_ind_surplus_heat=
1
Input_Period_ind_surplus_heat=
30
notes_model_areaText=
0.00
notes_model_yearText=
0.00
notes_developed_yearText=
0.00
general_notesText=
0.00
Filnavn_ind_surplus_heat=
const.txt
Filnavn_Hour_file_geo=
const.txt
Input_Inv_transport_bicycles=
0
Input_FOM_transport_bicycles=
0
Input_Period_transport_bicycles=
0
Input_Inv_transport_motorbikes=
0
Input_FOM_transport_motorbikes=
0
Input_Period_transport_motorbikes=
0
Input_Inv_transport_electric_cars=
28.1
Input_FOM_transport_electric_cars=
0.12
Input_Period_transport_electric_cars=
16
Input_Inv_transport_conventional_cars=
20.79
Input_FOM_transport_conventional_cars=
0.7
Input_Period_transport_conventional_cars=
16
Input_Inv_transport_electric_busses=
0
Input_FOM_transport_electric_busses=
0
Input_Period_transport_electric_busses=
0
Input_Inv_transport_diesel_busses=
183.75
Input_FOM_transport_diesel_busses=
0.55
Input_Period_transport_diesel_busses=
6
Input_Inv_transport_electric_trucks=
102.9
Input_FOM_transport_electric_trucks=
1.27
Input_Period_transport_electric_trucks=
6
Input_Inv_transport_diesel_trucks=
102.9
Input_FOM_transport_diesel_trucks=
1.27
Input_Period_transport_diesel_trucks=
6
Input_Inv_transport_other_vehicles1=
0
Input_FOM_transport_other_vehicles1=
0
Input_Period_transport_other_vehicles1=
0
Input_Inv_transport_other_vehicles2=
0
Input_FOM_transport_other_vehicles2=
0
Input_Period_transport_other_vehicles2=
0
Input_Inv_transport_other_vehicles3=
0
Input_FOM_transport_other_vehicles3=
0
Input_Period_transport_other_vehicles3=
0
Input_Inv_transport_other_vehicles4=
0
Input_FOM_transport_other_vehicles4=
0
Input_Period_transport_other_vehicles4=
0
Input_Inv_transport_other_vehicles5=
0
Input_FOM_transport_other_vehicles5=
0
Input_Period_transport_other_vehicles5=
0
Input_Size_transport_bicycles=
0
Input_Size_transport_motorbikes=
0
Input_Size_transport_electric_cars=
0
Input_Size_transport_conventional_cars=
0
Input_Size_transport_electric_busses=
0
Input_Size_transport_diesel_busses=
0
Input_Size_transport_electric_trucks=
0
Input_Size_transport_diesel_trucks=
0
Input_Size_transport_other_vehicles1=
0
Input_Size_transport_other_vehicles2=
0
Input_Size_transport_other_vehicles3=
0
Input_Size_transport_other_vehicles4=
0
Input_Size_transport_other_vehicles5=
0
other_vehicles1Text=
0.00
other_vehicles2Text=
0.00
other_vehicles3Text=
0.00
other_vehicles4Text=
0.00
other_vehicles5Text=
0.00
NameRES5=
Tidal
NameRES6=
Wave Power
NameRES7=
Wind
input_RES5_capacity=
0
input_RES5_factor=
0
input_RES6_capacity=
0
input_RES6_factor=
0
input_RES7_capacity=
0
input_RES7_factor=
0.9
input_RES5_stab_share=
0
input_RES6_stab_share=
0
input_RES7_stab_share=
0
Filnavn_RES5=
const.txt
Filnavn_RES6=
const.txt
Filnavn_RES7=
GRC Offshore wind.txt
input_cshp_th_own_gr1=
0
input_cshp_th_own_gr2=
0
input_cshp_th_own_gr3=
0
EmissionUnit=
Mt
Input_Inv_ind_CHP_elec=
0
Input_Period_ind_CHP_elec=
0
Input_FOM_ind_CHP_elec=
0
Input_Inv_ind_CHP_heat=
0
Input_Period_ind_CHP_heat=
0
Input_FOM_ind_CHP_heat=
0
input_Nuclear_partload=
1
input_Cooling_Chillers_demand=
1.2545
input_CoolingChillers_eff=
8.2
input_NaturalCooling_Chillers=
0.1631
input_Cooling_gr1_network_loss=
0
input_Cooling_gr2_network_loss=
0
input_Cooling_gr3_network_loss=
0.13
input_Cooling_Chiller_network_loss=
0.13
Filnavn_cooling_netloss=
const.txt
Input_V2G_TechnicalRegulation=
1
input_fuel_dhp[7]=
0
input_fuel_chp2[7]=
0
input_fuel_chp3[7]=
0
input_fuel_Boiler2[7]=
0
input_fuel_Boiler3[7]=
0
input_fuel_PP[7]=
0
input_fuel_PP2[7]=
0
Input_V2G_Hydro_Priotization=
1
input_eff_ELTCO2_fuel=
0.8
input_eff_ELTBiomass_fuel=
0.8
input_eff_ELTBiogas_fuel=
0.8
Input_CO2Elt_DHgr2_Share=
0
Input_CO2Elt_DHgr3_Share=
0.02
Input_BiomassElt_DHgr2_Share=
0
Input_BiomassElt_DHgr3_Share=
0.02
Input_BiogasElt_DHgr2_Share=
0
Input_BiogasElt_DHgr3_Share=
0
Input_transys=
1
input_cap_rock_el=
0
share_rock_store=
1
input_cap_rock_steam=
0
input_rock_store_cap=
0
input_rock_store_loss=
0.05
input_rockbed_reg=
1
input_HydroPowerStorageYearBegin=
0.5
input_HydroPowerStorageYearEnd=
0.5
input_HydroPowerContentButton=
0
input_rock_steam_output_eff=
1
input_VC_SteamStorage=
0
input_Inv_SteamStorage=
0
input_Period_SteamStorage=
0
input_FOM_SteamStorage=
0
Filnavn_CSP=
GRC Solar thermal.txt
Input_CSP_Solar=
0
Input_CSP_Storage_cap=
0
Input_CSP_Storage_eff=
0.5
Input_CSP_Power_cap=
0
Input_CSP_Power_eff=
0.3
input_CSP_stab_share=
0
ExcessHeatToSolarStorage=
False
Filnavn_Industry_Hydrogen=
const.txt
input_fuel_CSHP[6]=
3
input_eff_ELTIndustry_fuel=
0.8
Input_IndustryElt_DHgr2_Share=
0
Input_IndustryElt_DHgr3_Share=
0
Input_RESZeroOrNegativePrices=
2
Input_LiqHydroLiqFuel=
5.72
Input_LiqHydro_HydrogenShare=
0.49
Input_LiqHydro_eff=
0.81
Input_LiqMethanLiqFuel=
0
Input_LiqMethan_HydrogenShare=
0
Input_LiqMethan_eff=
0
Input_LiqCO2HydroHydrogenRatio=
1.19
Input_LiqCO2HydroSequestrationCO2Eff=
0.26
Input_CO2HydroLiqFuel=
11.44
Input_inv_LiqHydro=
0.3
Input_FOM_LiqHydro=
4
Input_Period_LiqHydro=
25
Input_inv_SynHydroBio=
0.2
Input_period_SynHydroBio=
25
Input_FOM_SynHydroBio=
4
Input_inv_LiqHydroBio=
0.3
Input_period_LiqHydroBio=
25
Input_FOM_LiqHydroBio=
4
Input_inv_SynMethan=
0
Input_period_SynMethan=
0
Input_FOM_SynMethan=
0
Input_inv_LiqMethan=
0
Input_period_LiqMethan=
0
Input_FOM_LiqMethan=
0
Input_inv_SynFuelPetrol=
0
Input_period_SynFuelPetrol=
0
Input_FOM_SynFuelPetrol=
0
Input_inv_SynFuelDiesel=
0
Input_period_SynFuelDiesel=
0
Input_FOM_SynFuelDiesel=
0
Input_SynHydro_DHgr2_Share=
0
Input_SynHydro_DHgr3_Share=
0.15
Input_SynMethane_DHgr2_Share=
0
Input_SynMethane_DHgr3_Share=
0.05
input_hp_maxload2=
0.5
Input_add_el_TWh=
15.75
Filnavn_add_el=
GRC Electricity demand.txt
Input_N2NH3Eff=
0.16
Input_H2NH3Eff=
1.15
Input_NH3Output=
0
Input_ElecN2Eff=
0.12
Input_NH3DH2Share=
0
Input_NH3DH3Share=
0
Input_NH3MaxCap=
0
Input_NH3EltEff_fuel=
0.8
Input_NH3Elt_DH2_share=
0
Input_NH3Elt_DH3_share=
0.05
Input_NH3_input=
1.49
Input_km_NH3=
1.5
Input_inv_N2_air=
0
Input_Period_N2_air=
0
Input_FOM_N2_air=
0
Input_Inv_NH3=
0
Input_Period_NH3=
0
Input_FOM_NH3=
0
input_cap_pump_el2=
2969.79
input_eff_pump_el2=
0.92
input_cap_turbine_el2=
2969.79
input_eff_turbine_el2=
0.92
input_storage_pump_cap2=
9.96
input_Inv_pump2=
0
input_Period_pump2=
0
input_FOM_pump2=
0
input_Inv_turbine2=
0
input_Period_turbine2=
0
input_FOM_turbine2=
0
input_Inv_PumpStorage2=
300
input_Period_PumpStorage2=
20
input_FOM_PumpStorage2=
0
Input_ThermalStorageRegulationGr3=
Weekly
Input_ThermalStorageRegulationGr2=
Weekly
Input_IncludeEB2=
No
Input_IncludeEB3=
No
Filnavn_WishImportExport=
zero.txt
Input_CAES_hour_time=
24
input_ElecStorProfitMargin=
0
MaxElectricityMarketPrice=
0
MinElectricityMarketPrice=
0
CHP_gridstab_priority=
false
input_CHP2_SO2=
0
input_CHP3_SO2=
0
input_Waste_SO2=
0
input_PP_SO2=
0
input_Nuclear_SO2=
0
input_Biogas_SO2=
0
input_Gasification_SO2=
0
input_HHCoal_SO2=
0
input_HHOil_SO2=
0
input_HHGas_SO2=
0
input_HHBio_SO2=
0
input_H2CHP_SO2=
0
input_GasCHP_SO2=
0
input_BioCHP_SO2=
0
input_CHP2_PM=
0
input_CHP3_PM=
0
input_Waste_PM=
0
input_PP_PM=
0
input_Nuclear_PM=
0
input_Biogas_PM=
0
input_Gasification_PM=
0
input_HHCoal_PM=
0
input_HHOil_PM=
0
input_HHGas_PM=
0
input_HHBio_PM=
0
input_H2CHP_PM=
0
input_GasCHP_PM=
0
input_BioCHP_PM=
0
input_CHP2_NO=
0
input_CHP3_NO=
0
input_Waste_NO=
0
input_PP_NO=
0
input_Nuclear_NO=
0
input_Biogas_NO=
0
input_Gasification_NO=
0
input_HHCoal_NO=
0
input_HHOil_NO=
0
input_HHGas_NO=
0
input_HHBio_NO=
0
input_H2CHP_NO=
0
input_GasCHP_NO=
0
input_BioCHP_NO=
0
input_CHP2_CH4=
0
input_CHP3_CH4=
0
input_Waste_CH4=
0
input_PP_CH4=
0
input_Nuclear_CH4=
0
input_Biogas_CH4=
0
input_Gasification_CH4=
0
input_HHCoal_CH4=
0
input_HHOil_CH4=
0
input_HHGas_CH4=
0
input_HHBio_CH4=
0
input_H2CHP_CH4=
0
input_GasCHP_CH4=
0
input_BioCHP_CH4=
0
input_CHP2_N2O=
0
input_CHP3_N2O=
0
input_Waste_N2O=
0
input_PP_N2O=
0
input_Nuclear_N2O=
0
input_Biogas_N2O=
0
input_Gasification_N2O=
0
input_HHCoal_N2O=
0
input_HHOil_N2O=
0
input_HHGas_N2O=
0
input_HHBio_N2O=
0
input_H2CHP_N2O=
0
input_GasCHP_N2O=
0
input_BioCHP_N2O=
0
input_HTL_Waste=
0
input_HTL_biomass=
0
input_HTL_eff_H2=
0.446
input_HTL_eff_JP=
0.205
input_HTL_eff_BioDiesel=
0.547
input_HTL_eff_Methanol=
0.288
input_HTL_eff_Syngas=
0.119
input_HTL_eff_DHGr3=
0.162
input_HTL_eff_InputToBiogas=
0.112
input_Pyrolysis_Waste=
0
input_Pyrolysis_Biomass=
0
input_Pyrolysis_eff_Syngas=
0.19
input_Pyrolysis_eff_BioDiesel=
0.15
input_Pyrolysis_eff_JP=
0.08
input_Pyrolysis_eff_BioChar=
0.4
input_Pyrolysis_eff_BiocharToCO2=
324
input_BiogasToPyrolysis=
0
input_HTL_eff_BioPetrol=
0.081
input_inv_htl=
0
input_FOM_htl=
0
input_period_htl=
0
input_inv_pyr=
0
input_FOM_pyr=
0
input_period_pyr=
0
xxx
xxx
xxx
xxx
xxx
xxx
xxx
xxx
xxx
xxx
